**Reinstatement Diagram – this must be completed and returned with Section 50 application.**

**Please complete with details of reinstatement materials and depths per each level, see example below.**

**Road Surface**

|  |  |  |
| --- | --- | --- |
|  |  |  |
|  |  |
|  |  |
|  |  |
| Surround to Apparatus |  |

Include depths and materials used for each section and total excavation depth.

Please see example illustrated below.

Please refer to Department for Transport New Roads and Street Works Act 1991 – Specification for the Reinstatement of Openings in Highways (Hauc Spec) for permitted variants.

<https://assets.publishing.service.gov.uk/government/uploads/system/uploads/attachment_data/file/11042/sroh.pdf>

**Example of Completed Reinstatement Diagram**

|  |  |  |
| --- | --- | --- |
| Approx. 2400mm TotalExcavation Depth | HRASC -Surface Course |  Minimum 40 mm |
| HRABC Base Course | Minimum 60 mm |
| GSB Type 1 Sub-base |  Minimum 150 mm |
| Imported Back Fill |  |
| Surround to Apparatus |  |

 **Road Surface**

Please refer to Department for Transport New Roads and Street Works Act 1991 – Specification for the Reinstatement of Openings in Highways (Hauc Spec) for permitted variants.

<https://assets.publishing.service.gov.uk/government/uploads/system/uploads/attachment_data/file/11042/sroh.pdf>